Contents - Previous - Next

Profile Settings - Monitoring

On this tab sheet, you specify whether invocation of the profile should be triggered by the presence of network paths or other devices such as USB drives.

The profile will be executed as soon as a drive becomes available, or as soon as this computer is connected to the LAN.

The presence of a drive is detected by simply trying to access it at regular intervals. Specify the delay between access attempts here. In addition, you will usually want the profile to pause for a longer time when it has run successfully. You can specify the pause after a successful run too.

The scheduler must be running for the monitoring to become active!

See also:

Upper Part Of Tab Seet

Advanced Settings